

**REMUS product information 05-2015**

**VW Golf VII type AU, SEAT Leon type 5F**

Dear **REMUS** Partner,

We are pleased to inform you that we have completed our next development

**REMUS sport exhaust and non-resonated RACING section with selectable tail pipes for the**

**VW Golf VII type AU and SEAT Leon type 5F**

It would be a pleasure for us to receive your order.

Stay tuned!

Your **REMUS** Team



**#83C: 2 tail pipes Ø 84 mm**

**Street Race, polished**

**#83CTS: 2 Carbon tail pipes Ø 84 mm angled, Titanium internals**

**#55S: 2 tail pipes Ø 84 mm, angled, chromed**

**#83CS: 2 tail pipes Ø 84 mm**

**Carbon Race, polished**

**#83CB: 2 tail pipes Ø 84 mm**

**Street Race Black Chrome**

|  |  |  |
| --- | --- | --- |
| **Car and engine specification** | | |
| **SEAT Leon, type 5F, 2013=>**  **SEAT Leon SC, type 5F, 2013=>**  **SEAT Leon FR, type 5F, 2013=>**  **SEAT Leon FR SC, type 5F, 2013=>**  1.2l TSI 63 kW (CJZB); 1.2l TSI 77 kW (CJZA); 1.4l TSI 90 kW (CMPA/CXSA); 1.4l TSI 103 kW (CHPA); 1.6l TDI 66 kW (CLHB); 1.8l TSI 132 kW (CJS); 1.6l TDI 77 kW (CLHA); 2.0l TDI 110 kW (CKFC); 2.0l TDI 135 kW (CUPA) | | |
| **Part no.** | **Description** | **€ RRP price excl. VAT** |
| **954112 0000** | Stainless steel connection tube (multi-link axle) for mounting on 1.8l TSI 132 kW, 2.0l TDI 110 kW, 2.0l TDI 135 kW | **55,--** |
| **953612 0000** | Stainless steel connection tube (twist beam axle) for mounting on 1.2l TSI 63 kW, 1.2l TSI 77 kW, 1.4l TSI 90 kW, 1.4l TSI 103 kW, 1.6l TDI 66 kW, 1.6l TDI 77 kW | **55,--** |
|  | | |
| **Sport exhaust system left, with EEC homologation:** | | |
| **953112 0584CS** | Stainless steel sport exhaust with 2 tail pipes Ø 84 mm Carbon Race, only for 1.2l TSI 63 kW; 1.2l TSI 77 kW; 1.4l TSI 90 kW; 1.4l TSI 103 kW; 1.8l TSI 132 kW | **399,--** |
| **954112 0584CS** | Stainless steel with 2 tail pipes Ø 84 mm Carbon Race, only for 1.6l TDI 66 kW; 1.6l TDI 77 kW; 2.0l TDI 110 kW; 2.0l TDI 135 kW | **399,--** |
|  | | |
| **Sport exhaust system centered, with EEC homologation:** | | |
| **794112 5536** | Stainless steel sport exhaust with 2 tail pipes 93x74 mm centered | **438,--** |
| **791302 HES** | ABS rear diffusor centered, carbon optic, for SEAT Leon/Leon SC | **191,--** |
| **791301 HES** | ABS rear diffusor centered, carbon optic, for SEAT Leon FR/Leon FR SC | **191,--** |
|  | | |
| **Sport exhaust system left/right, with selectable tail pipes, with EEC homologation:** | | |
| **955113 1500** | Stainless steel sport exhaust centered for L/R system (without tail pipes), Ø 70 mm tube, with EEC homologation | **280,--** |
| **alternative: Non-resonated RACING section left/right, with selectable tail pipes, without homologation:** | | |
| **954112 1600** | Stainless steel non-resonated RACING section L/R (without tail pipes), without homologation | **120,--** |
|  | | |
| **choose from following tail pipe package:** | | |
| **0046 55S** | tail pipe set L/R consisting of 4 tail pipes Ø 84 mm angled, chromed, with adjustable spherical clamp connection | **300,--** |
| **0046 83C** | tail pipe set L/R consisting of 4 tail pipes Ø 84 mm Street Race, with adjustable spherical clamp connection | **340,--** |
| **0046 83CS** | tail pipe set L/R consisting of 4 tail pipes Ø 84 mm Carbon Race, with adjustable spherical clamp connection | **360,--** |
| **0046 83CB** | tail pipe set L/R consisting of 4 tail pipes Ø 84 mm Street Race Black Chrome, with adjustable spherical clamp connection | **388,--** |
| **0046 83CTS** | tail pipe set 2 Carbon tail pipes Ø 84 mm angled, Titanium internals, with adjustable spherical clamp connection | **680,--** |
| **ATTENTION:**   * 955113 1500 and tail pipe package replaces part numbers 954112 1556 and 954112 1584C which will be available as long as stock lasts. * 954112 1600 and tail pipe package replaces part number 954112 1684C. * The sport exhausts respectively Racing section L/R are only mountable with connection tubes! * The sport exhaust left/right respectively Racing section L/R can only be installed using the above mentioned tip sets! * When fitting left or L/R system respectively Racing section L/R, the rear skirt must be trimmed as per the supplied template! * Sport exhaust centered & rear skirt only fits as a complete system! | | |

|  |  |  |
| --- | --- | --- |
| **Car and engine specification** | | |
| **VW Golf VII, type AU, 2012=>**  **VW Golf VII GTD, type AU, not for cars with sport & sound package, 2012=>**  1.2l TSI 63 kW (CJZB); 1.2l TSI 77 kW (CJJA); 1.4l TSI 90 kW (CMBA/CPVA); 1.4l TSI 103 kW (CHPA/CPTA); 1.6l TDI 66 kW (CLHB); 1.6l TDI 77 kW (CLHA); 2.0l TDI 81 kW (CRVA); 2.0l TDI 110 kW (CRBC); 2.0l GTD 135 kW (CUN) | | |
| **Part no.** | **Description** | **€ RRP price excl. VAT** |
| **954312 0000** | Stainless steel Racing tube without homologation, instead of front silencer, only for 1.4l TSI 90/103 kW | **155,--** |
|  | | |
| **954112 0000** | Stainless steel connection tube (multi-link axle) for mounting on 1.4l TSI 90 kW, 1.4l TSI 103 kW, 2.0l TDI 110 kW, 2.0l GTD 135 kW | **55,--** |
| **953612 0000** | Stainless steel connection tube (twist beam axle) for mounting on 1.2l TSI 63 kW, 1.2l TSI 77 kW, 1.6l TDI 66 kW, 1.6l TDI 77 kW, 2.0l TDI 81 kW | **55,--** |
|  | | |
| **Sport exhaust system left, with EEC homologation:** | | |
| **953112 0584CS** | Stainless steel sport exhaust with 2 tail pipes Ø 84 mm Carbon Race, only for 1.2l TSI 63 kW; 1.2l TSI 77 kW; 1.4l TSI 90 kW; 1.4l TSI 103 kW; | **399,--** |
| **954112 0584CS** | Stainless steel sport exhaust with 2 tail pipes Ø 84 mm Carbon Race, only for 1.6l TDI 66 kW; 1.6l TDI 77 kW; 2.0l TDI 81 kW; 2.0l TDI 110 kW; 2.0l GTD 135 kW | **399,--** |
|  | | |
| **Sport exhaust system left/right, with selectable tail pipes, with EEC homologation:** | | |
| **955113 1500** | Stainless steel sport exhaust centered for L/R system (without tail pipes), Ø 70 mm tube, with EEC homologation | **280,--** |
| **alternative: Non-resonated RACING section left/right, with selectable tail pipes, without homologation:** | | |
| **954112 1600** | Stainless steel non-resonated RACING section L/R (without tail pipes), without homologation | **120,--** |
|  | | |
| **951401 HES** | ABS rear diffusor left/right, carbon optic | **191,--** |
| **952401 HES** | ABS rear diffusor left/right, satin black | **191,--** |
|  | | |
| **choose from following tail pipe package:** | | |
| **0046 55S** | tail pipe set L/R consisting of 4 tail pipes Ø 84 mm angled, chromed, with adjustable spherical clamp connection | **300,--** |
| **0046 83C** | tail pipe set L/R consisting of 4 tail pipes Ø 84 mm Street Race, with adjustable spherical clamp connection | **340,--** |
| **0046 83CS** | tail pipe set L/R consisting of 4 tail pipes Ø 84 mm Carbon Race, with adjustable spherical clamp connection | **360,--** |
| **0046 83CB** | tail pipe set L/R consisting of 4 tail pipes Ø 84 mm Street Race Black Chrome, with adjustable spherical clamp connection | **388,--** |
| **0046 83CTS** | tail pipe set 2 Carbon tail pipes Ø 84 mm angled, Titanium internals, with adjustable spherical clamp connection | **680,--** |
| **ATTENTION:**   * 955113 1500 and tail pipe package replaces part numbers 954112 1556 and 954112 1584C which will be available as long as stock lasts. * 954112 1600 and tail pipe package replaces part number 954112 1684C. * The sport exhaust left/right respectively Racing section L/R can only be installed using the above mentioned tip sets! * The sport exhausts respectively Racing section L/R are only mountable with connection tubes! * The rear diffusors are only mountable together with the L/R systems respectively Racing section L/R. * Alternatively also the original rear skirt can be used but it has to be trimmed according to enclosed instructions! | | |

|  |  |  |
| --- | --- | --- |
| **Car and engine specification** | | |
| **VW Golf VII GTD, type AU,**  **for cars with sport & sound package, 2012=>**  2.0l GTD 135 kW (CUN) | | |
| **Part no.** | **Description** | **€ RRP price excl. VAT** |
| **954212 0000** | Stainless steel connection tube for mounting on 2.0l GTD 135 kW | **55,--** |
|  | | |
| **Non-resonated section left/right, with selectable tail pipes, with EEC homologation:** | | |
| **954112 1600** | Stainless steel non-resonated section L/R (without tail pipes), with EEC homologation | **120,--** |
|  | | |
| **951401 HES** | ABS rear diffusor left/right, carbon optic | **191,--** |
| **952401 HES** | ABS rear diffusor left/right, satin black | **191,--** |
|  | | |
| **choose from following tail pipe package:** | | |
| **0046 55S** | tail pipe set L/R consisting of 4 tail pipes Ø 84 mm angled, chromed, with adjustable spherical clamp connection | **300,--** |
| **0046 83C** | tail pipe set L/R consisting of 4 tail pipes Ø 84 mm Street Race, with adjustable spherical clamp connection | **340,--** |
| **0046 83CS** | tail pipe set L/R consisting of 4 tail pipes Ø 84 mm Carbon Race, with adjustable spherical clamp connection | **360,--** |
| **0046 83CB** | tail pipe set L/R consisting of 4 tail pipes Ø 84 mm Street Race Black Chrome, with adjustable spherical clamp connection | **388,--** |
| **0046 83CTS** | tail pipe set 2 Carbon tail pipes Ø 84 mm angled, Titanium internals, with adjustable spherical clamp connection | **680,--** |
| **ATTENTION :**   * 954112 1600 and tail pipe package replaces part number 954112 1684C. * L/R section can only be installed using the above mentioned tip sets! * L/R section is only mountable with connection tubes! * The rear diffusors are only mountable together with the L/R section. * The exhaust can only be installed using the original VW bracket 5Q0 253 144D! * Alternatively also the original rear skirt can be used but it has to be trimmed according to enclosed instructions! | | |

|  |  |  |
| --- | --- | --- |
| **Car and engine specification** | | |
| **VW Golf VII GTI / GTI Performance, type AU, 2013=>**  2.0l TSI 162 kW (CHH); 2.0l TSI 169 kW (CHH) | | |
| **Part no.** | **Description** | **€ RRP price excl. VAT** |
| **955113 1100** | Stainless steel RACING downpipe, tube Ø 70 mm, with sport catalytic convertor (200 CPSI), without homologation, can only be fitted in combination with the REMUS front silencer | **855,--** |
| **955113 0300** | Stainless steel front silencer, Ø 70 mm tube | **257,--** |
|  | | |
| **955213 0000** | Stainless steel connection tube for mounting on 2.0l TSI 162/169 kW | **55,--** |
|  | | |
| **Sport exhaust system left/right, with selectable tail pipes, with EEC homologation:** | | |
| **955113 1500** | Stainless steel sport exhaust centered for L/R system (without tail pipes), Ø 70 mm tube, with EEC homologation | **280,--** |
| **alternative: Non-resonated RACING section left/right, with selectable tail pipes, without homologation:** | | |
| **954112 1600** | Stainless steel non-resonated RACING section L/R (without tail pipes), without homologation | **120,--** |
|  | | |
| **951401 HES** | ABS rear diffusor left/right, carbon optic | **191,--** |
| **952401 HES** | ABS rear diffusor left/right, satin black | **191,--** |
|  | | |
| **choose from following tail pipe package:** | | |
| **0046 55S** | tail pipe set L/R consisting of 4 tail pipes Ø 84 mm angled, chromed, with adjustable spherical clamp connection | **300,--** |
| **0046 83C** | tail pipe set L/R consisting of 4 tail pipes Ø 84 mm Street Race, with adjustable spherical clamp connection | **340,--** |
| **0046 83CS** | tail pipe set L/R consisting of 4 tail pipes Ø 84 mm Carbon Race, with adjustable spherical clamp connection | **360,--** |
| **0046 83CB** | tail pipe set L/R consisting of 4 tail pipes Ø 84 mm Street Race Black Chrome, with adjustable spherical clamp connection | **388,--** |
| **0046 83CTS** | tail pipe set 2 Carbon tail pipes Ø 84 mm angled, Titanium internals, with adjustable spherical clamp connection | **680,--** |
| **ATTENTION:**   * 955113 1500 and tail pipe package replaces part numbers 954112 1556 and 954112 1584C which will be available as long as stock lasts. * 954112 1600 and tail pipe package replaces part number 954112 1684C. * The sport exhaust L/R respectively Racing section L/R can only be installed using the above mentioned tip sets! * The rear diffusors, L/R system respectively Racing section L/R and connection tube only fit as a complete system! | | |